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55-60kn Torque head - Spec Sheet 
Specification:
The 6000X has been designed for installing screw piles. The torque gauge fitted allows the user to monitor the installation torque as the piles are installed. The 8 bolt flange output allows a variety of adaptors to be fitted.

The 6000X torque head is designed to fit 8-30t excavators. This head will develop 60,000Nm torque at working pressures stated below- 
Technical Information Specifications 
· Max Pressure 300 Bar 
· Max Flow 150l/min 
· Max Speed 7rpm  
· Net Weight 480kg without cradle 
· Body Width 470mm  
· Powerhead length (from base to centre of pin) 1300mm 
· 2no Hydraulic hoses have ¾ inch BSP female fittings. 
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If you require any further technical information on the drive unit, please feel free to contact us on Info@ja-css.com 
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